Legend and Statistics

1 AC lands at Brussels RWY 25

1.1 CRW opts to continue landing

1.2 AC near Brussels Airport

1.1.1 CRW realizes they are landing at the wrong airport

1.1.2 CRW has safety reasons for continuing landing

1.1.3 Standard Operating Procedures

1.1.1.1 CRW gets visual contact to Brussels airport

1.1.1.2 CRW notices that Brussels’ airport layout is different from Frankfurt’s

1.1.1.1.1 AC breaks out under clouds

1.1.1.1.2 CRW procedures

2

1.2.1.3 CRW asks for the Bruno VOR’s frequency.

2.1.1 London received false data from SATC

1.2.2 AC cleared to BATC according to ATC procedures

1.2.1 CRW did not realize that they were on wrong course, UNTIL:[111]

1.2.1.2 ILS has different frequency for Frankfurt.

1.2.1.5 Situation remains safe during landing

1.2.1.6 Current approach plates are used

2.1 LATC procedures

2.2 LATC uses false flight data for NW052

3.1 SATC handoff procedures under this flightplan are to LATC

3.2 FI is correct at SATC

1.2.1.1 CRW addresses BATC controller as ‘‘Frankfurt’’ several times

1.2.1.4 Brussels did not question the addressing error although it happened more than once

3

4