1 self-destruct system of the launcher is triggered

1.1 launcher starts to disintegrate 1.3 specification and implementation of self-destruct system 1.2 boosters separate from main stage

1.1.1 high aerodynamic loads

1.1.1.1.1.1 OBC software commands nozzle deflections

1.1.1.1.1.1.1 OBC detects (imaginary) deviation from flightpath

1.1.1.1.1.1.2 OBC cannot switch to SRI 1

1.1.1.1.1.1.1.1 OBC receives partially improper flightdata from SRI 2

1.1.1.1.1.1.2.1 SRI 1 ceased working

1.1.1.1.1.1.2.1.1 software exception

1.1.1.1.1.1.2.1.1.1 Operand Error occurs

1.1.1.1.1.1.2.1.1.1.1 execution of a data conversion from 64-bit floating point to 16-bit signed integer

1.1.1.1.1.1.2.1.1.1.2 value of floating point number too high to be represented as 16-bit signed integer

1.1.1.1.1.1.2.1.1.1.3 concerned variable is unprotected

1.1.1.1.1.1.2.1.1.1.1.1 function not disabled, although it doesn’t serve any purpose after lift-off

1.1.1.1 high angle of attack (greater than 20 degrees)

1.1.1.1.1 full nozzle deflections of solid boosters and Vulcain main engine

1.1.1.1.1.1.1.1.1 bit-pattern is interpreted as flight-data

1.1.1.1.1.1.1.1.2 specification of OBC

1.1.1.1.1.1.1.1.1.1 SRI 2 sends diagnostic bit-pattern

1.1.1.1.1.1.1.1.1.2 specification of SRI

1.1.1.1.1.1.1.1.1.1.1 SRI 2 declares failure

1.1.1.1.1.1.2.1.1.1.1.1.2 alignment function is required for Ariane 4

1.1.1.1.1.1.2.1.1.1.2.1 value of BH is much higher than expected

1.1.1.1.1.1.2.1.1.1.2.1.1 early part of trajectory of Ariane 5 differs from that of Ariane 4

1.1.1.1.1.1.2.1.1.1.3.1 under consideration of Ariane 4 physics protection was unnecessary

1.1.1.1.1.1.2.1.1.1.3.2 use of Ariane 4 software

1.1.1.1.1.1.2.1.1.1.3.3 expectations based on Ariane 4 experiences

1.1.1.1.1.1.2.1.1.1.1.1.1 insufficient testing of this piece of software was done with Ariane 5 data